COMMENTS:
1. LAN NVM update package for AOC-ATG-i2T that uses Intel LAN X550-AT2 (17x17) and supports NCSI.
2. SSID 1b7d.
3. See Instruction.txt.

EEPROM REVISION INFO:
11) ATGi2T_X550_20250116_3-7_NUP (1/16/2025) - IPS 00931650.
	a. SMC-ATGi2T-dSGVL_B0_AT2_NCSI_3p70_0.10_800018A1.bin	
	b. NVM image is included with PXE3682.

4) ATGi2T2C_NUP (1/20/2022)
	a. SMC_dSGVL_B0_AT2_NCSI_3p50_80001743 ETrackID 80001743 from IPS 00673817.
	b. NVM image is included with PXE3082. 

3) ATGi2T2B_NUP (12/6/2021) - Fixed BMC Link Status
	a. SMC_dSGVL_B0_AT2_NCSI_3p50_80001738.bin ETrackID 80001738 from IPS 00665783.
	b. NVM image is included with PXE3082.
	c. NUP can update from all previous released version for this card – no transition is needed. 
	   1.93 (80000AEE), 2.10 (80000F49), 2.20 (80001112),  3.15 (80001373),  3.50 (800016DC). 

2) ATGi2T2A_NUP (10/21/2021)
	a. dSGVL_B0_AT2_NCSI_3p50_800016DC.bin ETrackID 800016DC.
	b. NVM image is included with PXE3082. 

1c) ATGi2T202_NUP (2/19/2020)
	a. Correct Map.txt for Link width
	b. Update cfg to update over ATGi2T201_NUP

1b) ATGi2T201_NUP (2/8/2020)
	a. Correct Link width.

1a) ATGi2T20_NUP (12/15/2020)
	a. Added Linux version. 

1) ATGi2T20_NUP (11/24/2020) - WILL NOT BE ABLE TO DOWNGRADE to older F/W version, ONCE UPGRADED to this F/W.
	a. UEFI NVM Update FW v3.15 ETrackID 80001373 (Intel dSGVL_B0_AT2_NCSI_3p15.bin). 
	b. Package is included BootIMG.FLB from PXE2829.