Steps to flash LAN EEPROM:

UEFI
	1. Extract the files and copy them to a USB.  
	2. Boot up UEFI Shell with USB plugged in.
	3. Go to your USB "fs0:".
	4. To update FW, execute "FWUpdate.nsh".
	5. AC off/on.

Linux_x64
	1. Make sure to have administrator privileges.
	2. If FWUpdate.sh and nvmupdate64e are NOT executeable, execute "chmod +x FWUpdate.sh nvmupdate64e".
	3. To update FW, execute "./FWUpdate.sh".
	4. Shutdown and then AC off-on.