In-band
fs0: flash.nsh [Target BMC FW] [UserName] [Password] [Current BMC Version] [Target BMC Version]
Ex: BMC_X12AST2600-NONROT-6301MS from 01.07.09 to 01.08.08
flash.nsh BMC_X12AST2600-NONROT-6301MS_20251212_01.08.08_STDsp.bin ADMIN ADMIN 010709 010808

Out-of-band
Linux SAA Revision: saa_1.4.0_Linux_x86_64
  ./flash_linux.sh [BMCIP] [Target BMC FW] [UserName] [Password] [Current BMC Version] [Target BMC Version]
Ex:BMC_X12AST2600-NONROT-6301MS from 01.07.09 to 01.08.08
./flash_linux.sh 10.11.22.33 BMC_X12AST2600-NONROT-6301MS_20251212_01.08.08_STDsp.bin ADMIN ADMIN 010709 010808
