================================================================================
Supermicro System IPMI Firmware Update Package Operation Instructions
================================================================================

Package Revision: 00.01
Revision of flash.nsh: 00.00.01
Date of flash.nsh: 2026-01-07
Revision of flash_linux.sh: 00.00.01      
Date of flash_linux.sh: 2026-01-07

Please read this document in it before performing the system IPMI firmware update.  
Please verify that your system meets the requirments.

********************************************************************************
This update package includes the following system software updates & utilities:

--- IPMI Firmware image ---

  IPMI Firmware                    - BMC_X13AST2600-NONROT-1501MS_20260222_01.09.05_STDsp.bin             (REV 01.09.05)
  Upgrade Transition Firmware      - BMC_X13AST2600-NONROT-1501MS_20250919_01.05.11_STDsp.bin             (REV 01.05.11)

  Important Notes: Due to security updates included in this release, downgrading to previous versions is not supported. This ensures your  
  system remains protected against known vulnerabilities.
  If you have a specific business requirement that necessitates downgrade to an older version, please contact Technical Support for guidance.

--- IPMI Firmware Update Tools ---

  SuperServer Automation Assistant (SAA) UEFI V1.4.0-p1 (2025/10/30)
 
  SAA.efi							(for UEFI)
  UEFI_SAA_UserGuide.pdf					(SAA UEFI UserGuide) 
  flash.nsh                                                     (Update Script)
  config.nsh			                                
  command_example.txt						(Example file for using the update script)


  SuperServer Automation Assistant (SAA) Linux V1.4.0 (2025/10/22)
 
  SAA							        (for Linux, under "saa_1.4.0_Linux_x86_64" folder)
  SAA_UserGuide.pdf					        (SAA Linux UserGuide, under "saa_1.4.0_Linux_x86_64" folder)
  SAA_PlatformFeatureSupportMatrix                              (under "saa_1.4.0_Linux_x86_64" folder)
  flash_linux.sh                                                (Update Script)
  config_files			                                
  command_example.txt						(Example file for using the update script)


--- Supported Products ---

  Supermicro Motherboards:
  MBD-X13SCW-F
  

*************************************************************************************
                       SYSTEM HARDWARE and FIRMWARE REQUIREMENTS
*************************************************************************************

<NONE>


*************************************************************************************
                                         Warning
*************************************************************************************

1. Do not interrupt, reboot or remove power from your system during the update.
   Doing so may cause the system failure.

2. If the software update fails, you may contact our RMA Department to have the BIOS/
   IPMI firmware chip reprogrammed.  This will require shipping the board to Supermicro
   for repair.  Please submit your RMA request at:
   http://www.supermicro.com/support/rma/.
