**SMC3008IR firmware Flash Process (PRELIMINARY 4/18/13)**

**Flashing IR mode in DOS mode:**

1) Please copy all files from DOS folder to bootable USB disk

2) Run SMC3008R.bat and following the instruction to enter the last 9 digits/character of the SAS address.

3) If you are having problem to enter the SAS address, please use the command below to set the controller SAS address.

 sas3flsh.exe -o –sasadd “Controller SAS address”

 For example: sas3flsh.exe -o –sasadd 50030480070a8b00

4) Reboot the system

**Flashing IR mode in UEFI mode**

1) Please copy all files from UEFI folder to bootable USB disk

2) Run SMC3008R.nsh and following the instruction to enter the last 9 digits/character of the SAS address.

3) If you are having problem to enter the SAS address, please use the command below to set the controller SAS address.

 sas3flash.efi -o –sasadd “Controller SAS address”

 For example: sas3flash.efi -o –sasadd 50030480070a8b00

4) Reboot the system